                      Ultima 6 AdLib/SoundBlaster Music Fix.


        To Install:     
                Make sure Ultima 6 is installed on your hard drive.
                Copy the U6ADLIB.DRV into your Ultima 6 directory. It
                will replace the old U6ADLIB.DRV music driver.
                EX: A:\COPY U6ADLIB.DRV C:\ULTIMA6

        Notes:  The Sound Blaster and AdLib require a 23microsecond delay
                after accessing the ports... In slower machines this was 
                not a problem. But sine machines like 486 and 586 are so
                quick, they do not delay the proper ammount of time need by 
                the AdLib/SB. Is what I did is inserted a delay which is 
                hooked to the 8253 Timer chip, which runs at 18.2Hz. This
                way it will delay the proper time, even on a 586.


        For Questions:

                Call Origin Customer Service
                at: 512-335-0440

                                        
